Driver-Rockey4-2.0.061122.x86.tar.gz

This ROCKEY4's Linux USB only driver are support all Linux's kernel v2.4 and above.

This driver is only support USB port dongle. 

For the existing customer who use this driver will need to recompile his/her application by using new library instead of their old object file from other version of ROCKEY's Linux driver which older than this version. 

Regarding to the new library file, after install the driver, you can find it in 　

            　/usr/local/lib/librockeyapi.a

    or 

             /usr/local/lib/librockeyapi.so


 

In the api directory both librockeyapi.so and librockeyapi.a are rockey4's library file, the first is static lib file,the second is dynamic lib file. Use anyone of the both 2 lib files is ok.

Makefile

test_so:
        gcc -o test_so test.c /usr/local/lib/librockeyapi.so

This line to compile test.c to be executable file use /usr/local/lib/librockeyapi.so.



test_a:
        gcc -o test_a test.c /usr/local/lib/librockeyapi.a

This line to compile test.c to be executable file use /usr/local/lib/librockeyapi.a.




support@rockey.com.my

www.rockey.com.my